|  |  |  |
| --- | --- | --- |
| ID | Date | Information |
| RF001 | 02/11/17 | The stakeholder didn´t give a specific time:   * The button has to be pressed at least 10 msec.   Meeting whit stakeholder |
| RF002 | 02/11/17 | The stakeholder didn´t give a sequence to detect the operation modes:   * In case than a valid button press is detected the module has to follow the next behavior depending on the button pressed.   Meeting whit stakeholder |
| RF004 | 02/11/17 | The stakeholder didn´t give information about the buttons. ¿What kind of buttons?   * The window shall UP until get totally CLOSED while the button keep press.   Meeting whit stakeholder |
| RF005 | 0/11/17 | The stakeholder didn´t give information about the buttons. ¿What kind of buttons?   * The window shall UP until get totally CLOSED automatically. (Function one touch).   Meeting whit stakeholder |
| RF006 | 02/11/17 | The stakeholder didn´t give information about the buttons. ¿What kind of buttons?   * The window shall DOWN until get totally OPEN while the button keep press.   Meeting whit stakeholder |
| RF007 | 02/11/17 | The stakeholder didn´t give information about the buttons. ¿What kind of buttons?   * The window shall DOWN until get totally OPEN automatically. (Function one touch).   Meeting whit stakeholder |
| RF008 | 02/11/17 | The stakeholder didn´t give information about the voltage level:   * It´s not specified   Meeting whit stakeholder |
| RF017 | 02/11/17 | The stakeholder didn´t give information about the indicator´s functionality (time)   * Each window movement has to be indicated trough a led color. Depending on movement each led has to be turn on.   Meeting whit stakeholder |
| RNF003 | 02/11/17 | The stakeholder didn´t give more information about the indicators   * It´s not specified   Meeting whit stakeholder |

|  |  |  |
| --- | --- | --- |
| ID | Date | Information |
| RNF013 | 02/11/17 | The stakeholder didn´t specific about a stop functionality:   * It´s not specified   Meeting whit stakeholder |
| RF018 | 02/11/17 | The stakeholder didn´t specific about a stop functionality |